IFC building model
Schema: "IFC2X3"
Description: "no view"
File name: "F:\Bimplus\Allplan Modell Bimplus Woche.ifc"
Time stamp: "2021-06-11T10:05:50"
Author: "Anke Niedermaier"
Organization: "No Organization"
Preprocessor: "EDMsix Version 2.0100.09 Sep 7 2016"
Originating system: "Allplan 2021.1 28.05.2021 - 12:51:35"
Application: "Allplan" version "2021.1" identifier "Allplan" by Organization "No Organization"

People and organizations
  Person "Anke" "Niedermaier" of Organization "No Organization"
  Owner history of Person "Anke" "Niedermaier" of Organization "No Organization" | application "Allplan" version "2021.1" identifier "Allplan" by Organization "No Organization" | change NOCHANGE | created 1623398741 (2021-06-11T08:05:41Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  MASSUNIT: KILO GRAM
  PLANEANGLEUNIT: DEGREE (conversion based)

Spatial structure
IFCPROJECT "Bimplus Woche"
  IFCSITE "Grundstück" | latitude 48° 8′ 10.319824″ | longitude 11° 41′ 19.319″
    contains 3 elements
      1 x IFCBUILDINGELEMENTPROXY | names: "" | material: "" | property sets: AllplanAttributes, AllplanQuantities
      2 x IFCBUILDINGELEMENTPROXY | object type "GeographicElement" | names: "" | material: "Erdreich"; "Rasen" | property sets: AllplanAttributes
    IFCBUILDING "Bürogebäude"
      contains 1 element
        1 x IFCBUILDINGELEMENTPROXY | object type "Chimney" | names: "Schornstein" | material: "Fertigteil Schornstein" | property sets: AllplanAttributes, Pset_BuildingElementProxyCommon
      IFCBUILDINGSTOREY "Gründung" | elevation -4.7
        contains 47 elements
          1 x IFCSLAB | BASESLAB | names: "Sauberkeitsschicht" | material: "C8/10" | property sets: AllplanAttributes, Pset_SlabCommon, AllplanQuantities, SlabQuantities
          11 x IFCFOOTING | STRIP_FOOTING | names: "Trägerrost" | material: "C25/30" | property sets: AllplanAttributes, Pset_FootingCommon, FootingQuantities
          35 x IFCFOOTING | PAD_FOOTING | names: "Bohrpfahl Gründung" | material: "C25/30" | property sets: AllplanAttributes, Pset_FootingCommon, FootingQuantities
      IFCBUILDINGSTOREY "Untergeschoss" | elevation -3.1
        contains 23 elements
          1 x IFCSLAB | BASESLAB | names: "" | material: "C25/30" | property sets: AllplanAttributes, Pset_SlabCommon, AllplanQuantities, SlabQuantities
          12 x IFCWALLSTANDARDCASE | names: "AW UG tr. Beton WU", "IW ntr. Beton", "IW tr. Beton" | material: layers ("C30/37 WU" 0.4, "Styrodur" 0.160000000000004); layers ("C30/37 WU" 0.4, "Styrodur" 0.16); layers ("C25/30" 0.2); layers ("C25/30" 0.4) | property sets: AllplanAttributes, Pset_WallCommon, WallQuantities
          9 x IFCCOLUMN | names: "Rechteckstütze UG" | material: "C30/37" | property sets: AllplanAttributes, Pset_ColumnCommon, AllplanQuantities, ColumnQuantities
          1 x IFCSTAIR | names: "Fertigteiltreppe" | material: "FT_STB C45" | property sets: AllplanAttributes, Pset_StairCommon
      IFCBUILDINGSTOREY "Erdgeschoss" | elevation -0.2
        contains 90 elements
          2 x IFCSLAB | FLOOR | names: "Geschossdecke", "Treppenpodest" | material: "C25/30" | property sets: AllplanAttributes, Pset_ManufacturerTypeInformation, Pset_SlabCommon, AllplanQuantities, SlabQuantities
          8 x IFCWALLSTANDARDCASE | names: "IW tr. Beton", "IW ntr. Beton" | material: layers ("C25/30" 0.4); layers ("C25/30" 0.2) | property sets: AllplanAttributes, Pset_WallCommon, WallQuantities
          2 x IFCSTAIR | names: "Fertigteiltreppe_I" | material: "FT_STB C45" | property sets: AllplanAttributes, Pset_StairCommon
          29 x IFCCOLUMN | names: "EG Stütze kurz", "EG Stütze lang" | material: "C30/37" | property sets: AllplanAttributes, Pset_ColumnCommon, AllplanQuantities, ColumnQuantities
          4 x IFCBEAM | names: "Unterzug lang", "Unterzug kurz" | material: "C30/37" | property sets: AllplanAttributes, Pset_BeamCommon, AllplanQuantities, BeamQuantities
          1 x IFCELEMENTASSEMBLY | names: "Eingangstüre" | parts: 5 IFCBUILDINGELEMENTPROXY | property sets: AllplanAttributes, Pset_ManufacturerTypeInformation
          44 x IFCCURTAINWALL | names: "Profil SN hoch", "Profil OW hoch", "Glaspaneel hoch" (+1 more) | material: "ALU ELOX"; "VSG" | property sets: AllplanAttributes, Pset_CurtainWallCommon, Pset_ManufacturerTypeInformation, AllplanQuantities
      IFCBUILDINGSTOREY "1. Obergeschoss" | elevation 4.9
        contains 87 elements
          1 x IFCSLAB | FLOOR | names: "Geschossdecke" | material: "C25/30" | property sets: AllplanAttributes, Pset_ManufacturerTypeInformation, Pset_SlabCommon, AllplanQuantities, SlabQuantities
          8 x IFCWALLSTANDARDCASE | names: "IW tr. Beton", "IW ntr. Beton" | material: layers ("C25/30" 0.4); layers ("C25/30" 0.2) | property sets: AllplanAttributes, Pset_WallCommon, WallQuantities
          4 x IFCBEAM | names: "Unterzug kurz", "Unterzug lang" | material: "C30/37" | property sets: AllplanAttributes, Pset_BeamCommon, AllplanQuantities, BeamQuantities
          1 x IFCSTAIR | names: "Fertigteiltreppe_II" | material: "FT_STB C45" | property sets: AllplanAttributes, Pset_StairCommon
          29 x IFCCOLUMN | names: "OG Stütze lang", "OG Stütze kurz" | material: "C30/37" | property sets: AllplanAttributes, Pset_ColumnCommon, AllplanQuantities, ColumnQuantities
          44 x IFCCURTAINWALL | names: "Profil SN standard", "Profil OW standard", "Glaspaneel standard" | material: "ALU ELOX"; "VSG" | property sets: AllplanAttributes, Pset_CurtainWallCommon, Pset_ManufacturerTypeInformation, AllplanQuantities
      IFCBUILDINGSTOREY "2. Obergeschoss" | elevation 8.6
        contains 108 elements
          1 x IFCSLAB | FLOOR | names: "Geschossdecke" | material: "C25/30" | property sets: AllplanAttributes, Pset_ManufacturerTypeInformation, Pset_SlabCommon, AllplanQuantities, SlabQuantities
          22 x IFCWALLSTANDARDCASE | names: "IW ntr. Beton", "IW tr. Beton", "GK_IW_Ausbau" | material: layers ("C25/30" 0.2); layers ("C25/30" 0.4); layers ("Gipskartonständerwand" 0.15); layers ("Gipskartonständerwand" 0.150000000000002) | property sets: AllplanAttributes, Pset_WallCommon, WallQuantities
          29 x IFCCOLUMN | names: "OG Stütze lang", "OG Stütze kurz" | material: "C30/37" | property sets: AllplanAttributes, Pset_ColumnCommon, AllplanQuantities, ColumnQuantities
          1 x IFCSTAIR | names: "Fertigteiltreppe_II" | material: "FT_STB C45" | property sets: AllplanAttributes, Pset_StairCommon
          4 x IFCBEAM | names: "Unterzug lang", "Unterzug kurz" | material: "C30/37" | property sets: AllplanAttributes, Pset_BeamCommon, AllplanQuantities, BeamQuantities
          44 x IFCCURTAINWALL | names: "Profil SN standard", "Profil OW standard", "Glaspaneel standard" | material: "ALU ELOX"; "VSG" | property sets: AllplanAttributes, Pset_CurtainWallCommon, AllplanQuantities, Pset_ManufacturerTypeInformation
          1 x IFCDOOR | type IFCDOORSTYLE "1flg Weiß Oberlicht" | names: "1flg Weiß Oberlicht" | material: "Innentür" | property sets: AllplanAttributes (1flg Weiß Oberlicht), AllplanQuantities, Pset_DoorCommon, Pset_ManufacturerTypeInformation
          1 x IFCDOOR | type IFCDOORSTYLE "1flg Weiß Oberlicht" | names: "1flg Weiß Oberlicht" | material: "Innentür" | property sets: AllplanAttributes (1flg Weiß Oberlicht), AllplanQuantities, Pset_DoorCommon, Pset_ManufacturerTypeInformation
          1 x IFCDOOR | type IFCDOORSTYLE "1flg Weiß Oberlicht" | names: "1flg Weiß Oberlicht" | material: "Innentür" | property sets: AllplanAttributes (1flg Weiß Oberlicht), AllplanQuantities, Pset_DoorCommon, Pset_ManufacturerTypeInformation
          1 x IFCDOOR | type IFCDOORSTYLE "1flg Weiß Oberlicht" | names: "1flg Weiß Oberlicht" | material: "Innentür" | property sets: AllplanAttributes (1flg Weiß Oberlicht), AllplanQuantities, Pset_DoorCommon, Pset_ManufacturerTypeInformation
          1 x IFCDOOR | type IFCDOORSTYLE "Türöffnung" | names: "Türöffnung" | material: "Innentür" | property sets: AllplanAttributes (Türöffnung), AllplanQuantities, Pset_DoorCommon, Pset_ManufacturerTypeInformation
          1 x IFCDOOR | type IFCDOORSTYLE "Türöffnung" | names: "Türöffnung" | material: "Innentür" | property sets: AllplanAttributes (Türöffnung), AllplanQuantities, Pset_DoorCommon, Pset_ManufacturerTypeInformation
          1 x IFCDOOR | type IFCDOORSTYLE "1flg Weiß Oberlicht" | names: "1flg Weiß Oberlicht" | material: "Innentür" | property sets: AllplanAttributes (1flg Weiß Oberlicht), AllplanQuantities, Pset_DoorCommon, Pset_ManufacturerTypeInformation
        IFCSPACE "VR/01" | long name "Vorraum Aufz./Treppe"
        IFCSPACE "TR/02 Treppenlauf" | long name "Treppe"
        IFCSPACE "INST/01" | long name "Installation"
        IFCSPACE "Raum 03" | long name "Büro" | INTERNAL
        IFCSPACE "TR/01 Treppenabsatz" | long name "Treppe"
        IFCSPACE "Raum 07" | long name "Empfang"
        IFCSPACE "Raum 08" | long name "Aufenthalt"
        IFCSPACE "Raum 09" | long name "Küche"
        IFCSPACE "Raum 01" | long name "Büro"
        IFCSPACE "Raum 11" | long name "WC Damen"
          contains 1 element
            1 x IFCCOVERING | FLOORING | names: "Hohlboden" | material: layers ("Hohlboden aufgeständert" 0.23, "Steinzeug" 0.02) | property sets: AllplanAttributes, AllplanQuantities, CoveringQuantities
        IFCSPACE "Raum 02" | long name "Büro"
        IFCSPACE "Raum 06" | long name "Büro"
        IFCSPACE "Raum 05" | long name "Büro"
        IFCSPACE "Raum 10" | long name "WC Herren"
          contains 1 element
            1 x IFCCOVERING | FLOORING | names: "Hohlboden" | material: layers ("Hohlboden aufgeständert" 0.23, "Steinzeug" 0.02) | property sets: AllplanAttributes, AllplanQuantities, CoveringQuantities
        IFCSPACE "AZ A/01" | long name "Aufzug A"
        IFCSPACE "AZ B/01" | long name "Aufzug B"
      IFCBUILDINGSTOREY "3. Obergeschoss" | elevation 12.3
        contains 108 elements
          1 x IFCSLAB | FLOOR | names: "Geschossdecke" | material: "C25/30" | property sets: AllplanAttributes, Pset_ManufacturerTypeInformation, Pset_SlabCommon, AllplanQuantities, SlabQuantities
          22 x IFCWALLSTANDARDCASE | names: "IW tr. Beton", "IW ntr. Beton", "GK_IW_Ausbau" | material: layers ("C25/30" 0.4); layers ("C25/30" 0.2); layers ("Gipskartonständerwand" 0.15); layers ("Gipskartonständerwand" 0.150000000000002) | property sets: AllplanAttributes, Pset_WallCommon, WallQuantities
          29 x IFCCOLUMN | names: "OG Stütze lang", "OG Stütze kurz" | material: "C30/37" | property sets: AllplanAttributes, Pset_ColumnCommon, AllplanQuantities, ColumnQuantities
          1 x IFCSTAIR | names: "Fertigteiltreppe_II" | material: "FT_STB C45" | property sets: AllplanAttributes, Pset_StairCommon
          4 x IFCBEAM | names: "Unterzug lang", "Unterzug kurz" | material: "C30/37" | property sets: AllplanAttributes, Pset_BeamCommon, AllplanQuantities, BeamQuantities
          44 x IFCCURTAINWALL | names: "Profil SN standard", "Profil OW standard", "Glaspaneel standard" | material: "ALU ELOX"; "VSG" | property sets: AllplanAttributes, Pset_CurtainWallCommon, AllplanQuantities, Pset_ManufacturerTypeInformation
          1 x IFCDOOR | type IFCDOORSTYLE "Türöffnung" | names: "Türöffnung" | material: "Innentür" | property sets: AllplanAttributes (Türöffnung), AllplanQuantities, Pset_DoorCommon, Pset_ManufacturerTypeInformation
          1 x IFCDOOR | type IFCDOORSTYLE "Türöffnung" | names: "Türöffnung" | material: "Innentür" | property sets: AllplanAttributes (Türöffnung), AllplanQuantities, Pset_DoorCommon, Pset_ManufacturerTypeInformation
          1 x IFCDOOR | type IFCDOORSTYLE "1flg Weiß Oberlicht" | names: "1flg Weiß Oberlicht" | material: "Innentür" | property sets: AllplanAttributes (1flg Weiß Oberlicht), AllplanQuantities, Pset_DoorCommon, Pset_ManufacturerTypeInformation
          1 x IFCDOOR | type IFCDOORSTYLE "1flg Weiß Oberlicht" | names: "1flg Weiß Oberlicht" | material: "Innentür" | property sets: AllplanAttributes (1flg Weiß Oberlicht), AllplanQuantities, Pset_DoorCommon, Pset_ManufacturerTypeInformation
          1 x IFCDOOR | type IFCDOORSTYLE "1flg Weiß Oberlicht" | names: "1flg Weiß Oberlicht" | material: "Innentür" | property sets: AllplanAttributes (1flg Weiß Oberlicht), AllplanQuantities, Pset_DoorCommon, Pset_ManufacturerTypeInformation
          1 x IFCDOOR | type IFCDOORSTYLE "1flg Weiß Oberlicht" | names: "1flg Weiß Oberlicht" | material: "Innentür" | property sets: AllplanAttributes (1flg Weiß Oberlicht), AllplanQuantities, Pset_DoorCommon, Pset_ManufacturerTypeInformation
          1 x IFCDOOR | type IFCDOORSTYLE "1flg Weiß Oberlicht" | names: "1flg Weiß Oberlicht" | material: "Innentür" | property sets: AllplanAttributes (1flg Weiß Oberlicht), AllplanQuantities, Pset_DoorCommon, Pset_ManufacturerTypeInformation
        IFCSPACE "INST/01" | long name "Installation"
        IFCSPACE "TR/02 Treppenlauf" | long name "Treppe"
        IFCSPACE "VR/01" | long name "Vorraum Aufz./Treppe"
        IFCSPACE "Raum 03" | long name "Büro" | INTERNAL
        IFCSPACE "Raum 10" | long name "WC Herren"
          contains 1 element
            1 x IFCCOVERING | FLOORING | names: "Hohlboden" | material: layers ("Hohlboden aufgeständert" 0.23, "Steinzeug" 0.02) | property sets: AllplanAttributes, AllplanQuantities, CoveringQuantities
        IFCSPACE "Raum 05" | long name "Büro"
        IFCSPACE "Raum 06" | long name "Büro"
        IFCSPACE "Raum 02" | long name "Büro"
        IFCSPACE "Raum 11" | long name "WC Damen"
          contains 1 element
            1 x IFCCOVERING | FLOORING | names: "Hohlboden" | material: layers ("Hohlboden aufgeständert" 0.23, "Steinzeug" 0.02) | property sets: AllplanAttributes, AllplanQuantities, CoveringQuantities
        IFCSPACE "Raum 01" | long name "Büro"
        IFCSPACE "Raum 09" | long name "Küche"
        IFCSPACE "Raum 08" | long name "Aufenthalt"
        IFCSPACE "Raum 07" | long name "Empfang"
        IFCSPACE "TR/01 Treppenabsatz" | long name "Treppe"
        IFCSPACE "AZ A/01" | long name "Aufzug A"
        IFCSPACE "AZ B/01" | long name "Aufzug B"
      IFCBUILDINGSTOREY "4. Obergeschoss" | elevation 16.
        contains 86 elements
          1 x IFCSLAB | FLOOR | names: "Geschossdecke" | material: "C25/30" | property sets: AllplanAttributes, Pset_ManufacturerTypeInformation, Pset_SlabCommon, AllplanQuantities, SlabQuantities
          8 x IFCWALLSTANDARDCASE | names: "IW ntr. Beton", "IW tr. Beton" | material: layers ("C25/30" 0.2); layers ("C25/30" 0.4) | property sets: AllplanAttributes, Pset_WallCommon, WallQuantities
          29 x IFCCOLUMN | names: "OG Stütze lang", "OG Stütze kurz" | material: "C30/37" | property sets: AllplanAttributes, Pset_ColumnCommon, AllplanQuantities, ColumnQuantities
          4 x IFCBEAM | names: "Unterzug lang", "Unterzug kurz" | material: "C30/37" | property sets: AllplanAttributes, Pset_BeamCommon, AllplanQuantities, BeamQuantities
          44 x IFCCURTAINWALL | names: "Profil SN standard", "Profil OW standard", "Glaspaneel standard" | material: "ALU ELOX"; "VSG" | property sets: AllplanAttributes, Pset_CurtainWallCommon, Pset_ManufacturerTypeInformation, AllplanQuantities
      IFCBUILDINGSTOREY "Dachgeschoss" | elevation 19.5
        contains 10 elements
          4 x IFCWALLSTANDARDCASE | names: "IW ntr. Beton" | material: layers ("C25/30" 0.2) | property sets: AllplanAttributes, Pset_WallCommon, WallQuantities
          1 x IFCSLAB | FLOOR | names: "Geschossdecke" | material: "C25/30" | property sets: AllplanAttributes, Pset_ManufacturerTypeInformation, Pset_SlabCommon, AllplanQuantities, SlabQuantities
          1 x IFCCOVERING | names: "" | material: "" | property sets: AllplanAttributes, PsetCoveringCommon, CoveringQuantities
          4 x IFCCURTAINWALL | names: "Profil OW standard" | material: "ALU ELOX" | property sets: AllplanAttributes, Pset_CurtainWallCommon, Pset_ManufacturerTypeInformation, AllplanQuantities

Types
  IFCDOORSTYLE "1flg Weiß Oberlicht" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "1flg Weiß Oberlicht" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "1flg Weiß Oberlicht" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "1flg Weiß Oberlicht" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "Türöffnung" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "Türöffnung" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "1flg Weiß Oberlicht" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "Türöffnung" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "Türöffnung" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "1flg Weiß Oberlicht" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "1flg Weiß Oberlicht" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "1flg Weiß Oberlicht" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "1flg Weiß Oberlicht" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCDOORSTYLE "1flg Weiß Oberlicht" | SINGLE_SWING_RIGHT | 1 occurrence

Property sets
  AllplanAttributes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Allright_Bauteil_ID = "0002ErE0000000071" (IFCTEXT)
    Einheit = "m³" (IFCTEXT)
    Objektname = "Quader" (IFCTEXT)
  AllplanAttributes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Allright_Bauteil_ID = "0002De 0000000003" (IFCTEXT)
    Außenbauteil = TRUE (IFCBOOLEAN)
    Codetext = "GEL 00" (IFCTEXT)
    Einheit = "m²" (IFCTEXT)
    Funktion = "Gelände" (IFCTEXT)
    Material = "Erdreich" (IFCTEXT)
    Objektname = "Gelände" (IFCTEXT)
    Umbaukategorie = "Neubau" (IFCTEXT)
    statisch_tragend = FALSE (IFCBOOLEAN)
  AllplanAttributes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Object Layer Attributes #1: Gewerk = "" (IFCTEXT); Schichtnummer = 1 (IFCINTEGER); Schichtdicke = 100. (IFCREAL); Dicke = 0. (IFCREAL); Faktor = 1. (IFCREAL); Objektname = "Belag" (IFCTEXT); Material = "Rasen" (IFCTEXT); Bezugshöhe = 0. (IFCREAL); Deltahöhe = 0. (IFCREAL); Allright_Bauteil_ID = "0002Bfl0000000004/01" (IFCTEXT); Einheit = "m²" (IFCTEXT)
  AllplanAttributes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Allright_Bauteil_ID = "0102Sch0000000041" (IFCTEXT)
    Außenbauteil = TRUE (IFCBOOLEAN)
    Bezeichnung = "Schornstein" (IFCTEXT)
    Breite_Lüftung = 105. (IFCREAL)
    Breite_Lüftung2 = 105. (IFCREAL)
    Dicke_Lüftung = 170. (IFCREAL)
    Dicke_Lüftung2 = 170. (IFCREAL)
    Einheit = "m" (IFCTEXT)
    Feuerwiderstandsklasse = "F30" (IFCTEXT)
    Gewerk = "Mauerarbeiten" (IFCTEXT)
    Material = "Fertigteil Schornstein" (IFCTEXT)
    Objektname = "Kamin" (IFCTEXT)
    Radius_Zug = 250. (IFCREAL)
    U-Wert = "0.80" (IFCTEXT)
    Umbaukategorie = "Neubau" (IFCTEXT)
    Zügigkeit = "1" (IFCTEXT)
    statisch_tragend = FALSE (IFCBOOLEAN)
  AllplanAttributes | properties | on 1 object (1 IFCSLAB)
    Allright_Bauteil_ID = "2001PFu0000000031" (IFCTEXT)
    Bezeichnung = "Sauberkeitsschicht" (IFCTEXT)
    Einheit = "m²" (IFCTEXT)
    Erdreich = "yes" (IFCTEXT)
    Gewerk = "Betonarbeiten" (IFCTEXT)
    Material = "C8/10" (IFCTEXT)
    Objektname = "Fundament" (IFCTEXT)
    Umbaukategorie = "Neubau" (IFCTEXT)
  AllplanAttributes | properties | on 1 object (1 IFCFOOTING)
    Allright_Bauteil_ID = "2002SFu0000000033" (IFCTEXT)
    Außenbauteil = TRUE (IFCBOOLEAN)
    Bezeichnung = "Trägerrost" (IFCTEXT)
    Einheit = "m³" (IFCTEXT)
    Erdreich = "yes" (IFCTEXT)
    Gewerk = "Betonarbeiten" (IFCTEXT)
    Lage (innen/außen) = 0 (IFCINTEGER)
    Material = "C25/30" (IFCTEXT)
    Objektname = "Fundament" (IFCTEXT)
  AllplanAttributes | properties | on 1 object (1 IFCFOOTING)
    Allright_Bauteil_ID = "2002SFu0000000029" (IFCTEXT)
    Außenbauteil = TRUE (IFCBOOLEAN)
    Bezeichnung = "Trägerrost" (IFCTEXT)
    Einheit = "m³" (IFCTEXT)
    Erdreich = "yes" (IFCTEXT)
    Gewerk = "Betonarbeiten" (IFCTEXT)
    Lage (innen/außen) = 0 (IFCINTEGER)
    Material = "C25/30" (IFCTEXT)
    Objektname = "Streifenfundament" (IFCTEXT)
  AllplanAttributes | properties | on 1 object (1 IFCFOOTING)
    Allright_Bauteil_ID = "2002SFu0000000055" (IFCTEXT)
    Außenbauteil = TRUE (IFCBOOLEAN)
    Bezeichnung = "Trägerrost" (IFCTEXT)
    Einheit = "m³" (IFCTEXT)
    Erdreich = "yes" (IFCTEXT)
    Gewerk = "Betonarbeiten" (IFCTEXT)
    Lage (innen/außen) = 0 (IFCINTEGER)
    Material = "C25/30" (IFCTEXT)
    Objektname = "Streifenfundament" (IFCTEXT)
  AllplanAttributes: 648 more contents on 648 objects not shown
  AllplanQuantities | quantities | on 160 objects (160 IFCCURTAINWALL)
    GrossSideArea = 13.693 [SQUARE_METRE]
  AllplanQuantities | quantities | on 154 objects (154 IFCCOLUMN)
    Length = 0.4 [METRE]
    Width = 0.4 [METRE]
  AllplanQuantities | quantities | on 39 objects (39 IFCCURTAINWALL)
    GrossSideArea = 19.867 [SQUARE_METRE]
  AllplanQuantities | quantities | on 24 objects (24 IFCOPENINGELEMENT)
    Depth = 0.2 [METRE]
    Height = 2.21 [METRE]
    Width = 1.21 [METRE]
  AllplanQuantities | quantities | on 20 objects (20 IFCBEAM)
    Height = 0.4 [METRE]
    Width = 0.4 [METRE]
  AllplanQuantities | quantities | on 12 objects (12 IFCOPENINGELEMENT)
    Depth = 0.4 [METRE]
    Height = 2.21 [METRE]
    Width = 1.21 [METRE]
  AllplanQuantities | quantities | on 10 objects (10 IFCOPENINGELEMENT)
    Depth = 0.15 [METRE]
    Height = 2.86 [METRE]
    Width = 1.26 [METRE]
  AllplanQuantities | properties | on 10 objects (10 IFCDOOR)
    DeductionOpeningBottom = 0. (IFCREAL)
    DeductionOpeningLeft = 70. (IFCREAL)
    DeductionOpeningRight = 70. (IFCREAL)
    DeductionOpeningTop = 70. (IFCREAL)
    GlassSurface = 0.336 (IFCREAL)
    HeightWindowSillInside = 0. (IFCREAL)
    HeightWindowSillOutside = 0. (IFCREAL)
    OffsetOpeningBottom = 250. (IFCREAL)
    OffsetOpeningLeft = 0. (IFCREAL)
    OffsetOpeningRight = 0. (IFCREAL)
    OffsetOpeningTop = 0. (IFCREAL)
  AllplanQuantities: 30 more contents on 82 objects not shown
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "FT_KAMM_1ZUG" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 6 objects (6 IFCSLAB)
    AcousticRating = "1" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Compartmentation = TRUE (IFCBOOLEAN)
    FireRating = "F120" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "DE_FT" (IFCIDENTIFIER)
    SurfaceSpreadOfFlame = "0.000000" (IFCLABEL)
    ThermalTransmittance = 0.55 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "FU_SSCH_KIE" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "FU_BPL" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  SlabQuantities | quantities | on 3 objects (3 IFCSLAB)
    GrossArea = 620.16 [SQUARE_METRE]
    GrossVolume = 124.032 [CUBIC_METRE]
    NetArea = 592.11 [SQUARE_METRE]
    NetVolume = 118.422 [CUBIC_METRE]
    NominalWidth = 0.2 [METRE]
  SlabQuantities | quantities | on 1 object (1 IFCSLAB)
    GrossArea = 661.44 [SQUARE_METRE]
    GrossVolume = 66.144 [CUBIC_METRE]
    NetArea = 661.44 [SQUARE_METRE]
    NetVolume = 66.144 [CUBIC_METRE]
    NominalWidth = 0.1 [METRE]
  SlabQuantities | quantities | on 1 object (1 IFCSLAB)
    GrossArea = 620.16 [SQUARE_METRE]
    GrossVolume = 248.064 [CUBIC_METRE]
    NetArea = 620.16 [SQUARE_METRE]
    NetVolume = 248.064 [CUBIC_METRE]
    NominalWidth = 0.4 [METRE]
  SlabQuantities | quantities | on 1 object (1 IFCSLAB)
    GrossArea = 620.16 [SQUARE_METRE]
    GrossVolume = 186.048 [CUBIC_METRE]
    NetArea = 591.34 [SQUARE_METRE]
    NetVolume = 177.402 [CUBIC_METRE]
    NominalWidth = 0.3 [METRE]
  SlabQuantities | quantities | on 1 object (1 IFCSLAB)
    GrossArea = 4.75 [SQUARE_METRE]
    GrossVolume = 0.95 [CUBIC_METRE]
    NetArea = 4.75 [SQUARE_METRE]
    NetVolume = 0.95 [CUBIC_METRE]
    NominalWidth = 0.2 [METRE]
  SlabQuantities | quantities | on 1 object (1 IFCSLAB)
    GrossArea = 620.16 [SQUARE_METRE]
    GrossVolume = 124.032 [CUBIC_METRE]
    NetArea = 592.94 [SQUARE_METRE]
    NetVolume = 118.588 [CUBIC_METRE]
    NominalWidth = 0.2 [METRE]
  SlabQuantities | quantities | on 1 object (1 IFCSLAB)
    GrossArea = 620.16 [SQUARE_METRE]
    GrossVolume = 186.048 [CUBIC_METRE]
    NetArea = 619.862 [SQUARE_METRE]
    NetVolume = 185.959 [CUBIC_METRE]
    NominalWidth = 0.3 [METRE]
  Pset_FootingCommon | properties | on 35 objects (35 IFCFOOTING)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "FU_GR_PFAHL" (IFCIDENTIFIER)
    Status = "Neubau" (IFCLABEL)
  Pset_FootingCommon | properties | on 4 objects (4 IFCFOOTING)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "FU_STR_LG" (IFCIDENTIFIER)
    Status = "Neubau" (IFCLABEL)
  Pset_FootingCommon | properties | on 3 objects (3 IFCFOOTING)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "FU_STR_KL" (IFCIDENTIFIER)
    Status = "Neubau" (IFCLABEL)
  Pset_FootingCommon | properties | on 2 objects (2 IFCFOOTING)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "FU_STR_Q" (IFCIDENTIFIER)
    Status = "Neubau" (IFCLABEL)
  Pset_FootingCommon | properties | on 2 objects (2 IFCFOOTING)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "FU_STR_RD" (IFCIDENTIFIER)
    Status = "Neubau" (IFCLABEL)
  FootingQuantities | quantities | on 35 objects (35 IFCFOOTING)
    GrossVolume = 7.012 [CUBIC_METRE]
    Height = 6.2 [METRE]
    Length = 1.195 [METRE]
    NetVolume = 7.012 [CUBIC_METRE]
    OuterSurfaceArea = 1.131 [SQUARE_METRE]
    Width = 0.946 [METRE]
  FootingQuantities | quantities | on 4 objects (4 IFCFOOTING)
    GrossVolume = 27.072 [CUBIC_METRE]
    Height = 1.2 [METRE]
    Length = 18.8 [METRE]
    NetVolume = 27.072 [CUBIC_METRE]
    OuterSurfaceArea = 22.56 [SQUARE_METRE]
    Width = 1.2 [METRE]
  FootingQuantities | quantities | on 3 objects (3 IFCFOOTING)
    GrossVolume = 12.672 [CUBIC_METRE]
    Height = 1.2 [METRE]
    Length = 8.8 [METRE]
    NetVolume = 12.672 [CUBIC_METRE]
    OuterSurfaceArea = 10.56 [SQUARE_METRE]
    Width = 1.2 [METRE]
  FootingQuantities | quantities | on 2 objects (2 IFCFOOTING)
    GrossVolume = 41.472 [CUBIC_METRE]
    Height = 1.2 [METRE]
    Length = 28.8 [METRE]
    NetVolume = 41.472 [CUBIC_METRE]
    OuterSurfaceArea = 34.56 [SQUARE_METRE]
    Width = 1.2 [METRE]
  FootingQuantities | quantities | on 2 objects (2 IFCFOOTING)
    GrossVolume = 30.528 [CUBIC_METRE]
    Height = 1.2 [METRE]
    Length = 21.2 [METRE]
    NetVolume = 30.528 [CUBIC_METRE]
    OuterSurfaceArea = 25.44 [SQUARE_METRE]
    Width = 1.2 [METRE]
  Pset_WallCommon | properties | on 28 objects (28 IFCWALLSTANDARDCASE)
    AcousticRating = "5" (IFCLABEL)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating = "F90" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "WA_TR_GK" (IFCIDENTIFIER)
    SurfaceSpreadOfFlame = "A" (IFCLABEL)
    ThermalTransmittance = 0.7 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 20 objects (20 IFCWALLSTANDARDCASE)
    AcousticRating = "4" (IFCLABEL)
    Compartmentation = TRUE (IFCBOOLEAN)
    FireRating = "F90" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "BT_WA_TR" (IFCIDENTIFIER)
    SurfaceSpreadOfFlame = "A" (IFCLABEL)
    ThermalTransmittance = 0.45 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 8 objects (8 IFCWALLSTANDARDCASE)
    AcousticRating = "4" (IFCLABEL)
    Compartmentation = TRUE (IFCBOOLEAN)
    FireRating = "F90" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BT_WA_NTR" (IFCIDENTIFIER)
    SurfaceSpreadOfFlame = "A" (IFCLABEL)
    ThermalTransmittance = 0.45 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 8 objects (8 IFCWALLSTANDARDCASE)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
  Pset_WallCommon | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    AcousticRating = "4" (IFCLABEL)
    Compartmentation = TRUE (IFCBOOLEAN)
    FireRating = "F90" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "KL_WA_TR" (IFCIDENTIFIER)
    SurfaceSpreadOfFlame = "A" (IFCLABEL)
    ThermalTransmittance = 0.45 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    AcousticRating = "4" (IFCLABEL)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating = "F90" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BT_WA_NTR" (IFCIDENTIFIER)
    SurfaceSpreadOfFlame = "B" (IFCLABEL)
    ThermalTransmittance = 0.45 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    AcousticRating = "4" (IFCLABEL)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating = "F90" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BT_WA_NTR" (IFCIDENTIFIER)
    SurfaceSpreadOfFlame = "A" (IFCLABEL)
    ThermalTransmittance = 0.45 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    AcousticRating = "4" (IFCLABEL)
    Compartmentation = TRUE (IFCBOOLEAN)
    FireRating = "F90" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "BT_WA_TR" (IFCIDENTIFIER)
    SurfaceSpreadOfFlame = "A" (IFCLABEL)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon: 1 more content on 4 objects not shown
  WallQuantities | quantities | on 14 objects (14 IFCWALLSTANDARDCASE)
    GrossFootprintArea = 0.69 [SQUARE_METRE]
    GrossSideArea = 16.1 [SQUARE_METRE]
    GrossSideAreaLeft = 16.1 [SQUARE_METRE]
    GrossVolume = 2.415 [CUBIC_METRE]
    NetSideArea = 16.1 [SQUARE_METRE]
    NetSideAreaLeft = 16.1 [SQUARE_METRE]
    NetVolume = 2.415 [CUBIC_METRE]
    NominalHeight = 3.5 [METRE]
    NominalLength = 4.6 [METRE]
    NominalWidth = 0.15 [METRE]
  WallQuantities | quantities | on 10 objects (10 IFCWALLSTANDARDCASE)
    GrossFootprintArea = 0.69 [SQUARE_METRE]
    GrossSideArea = 16.1 [SQUARE_METRE]
    GrossSideAreaLeft = 16.1 [SQUARE_METRE]
    GrossVolume = 2.415 [CUBIC_METRE]
    NetSideArea = 12.496 [SQUARE_METRE]
    NetSideAreaLeft = 12.496 [SQUARE_METRE]
    NetVolume = 1.874 [CUBIC_METRE]
    NominalHeight = 3.5 [METRE]
    NominalLength = 4.6 [METRE]
    NominalWidth = 0.15 [METRE]
  WallQuantities | quantities | on 8 objects (8 IFCWALLSTANDARDCASE)
    GrossFootprintArea = 0.92 [SQUARE_METRE]
    GrossSideArea = 16.1 [SQUARE_METRE]
    GrossSideAreaLeft = 16.1 [SQUARE_METRE]
    GrossVolume = 3.22 [CUBIC_METRE]
    NetSideArea = 10.752 [SQUARE_METRE]
    NetSideAreaLeft = 10.752 [SQUARE_METRE]
    NetVolume = 2.15 [CUBIC_METRE]
    NominalHeight = 3.5 [METRE]
    NominalLength = 4.6 [METRE]
    NominalWidth = 0.2 [METRE]
  WallQuantities | quantities | on 4 objects (4 IFCWALLSTANDARDCASE)
    GrossFootprintArea = 4. [SQUARE_METRE]
    GrossSideArea = 35. [SQUARE_METRE]
    GrossSideAreaLeft = 35. [SQUARE_METRE]
    GrossVolume = 14. [CUBIC_METRE]
    NetSideArea = 32.326 [SQUARE_METRE]
    NetSideAreaLeft = 32.326 [SQUARE_METRE]
    NetVolume = 12.93 [CUBIC_METRE]
    NominalHeight = 3.5 [METRE]
    NominalLength = 10. [METRE]
    NominalWidth = 0.4 [METRE]
  WallQuantities | quantities | on 4 objects (4 IFCWALLSTANDARDCASE)
    GrossFootprintArea = 2.16 [SQUARE_METRE]
    GrossSideArea = 18.9 [SQUARE_METRE]
    GrossSideAreaLeft = 18.9 [SQUARE_METRE]
    GrossVolume = 7.56 [CUBIC_METRE]
    NetSideArea = 18.9 [SQUARE_METRE]
    NetSideAreaLeft = 18.9 [SQUARE_METRE]
    NetVolume = 7.56 [CUBIC_METRE]
    NominalHeight = 3.5 [METRE]
    NominalLength = 5.4 [METRE]
    NominalWidth = 0.4 [METRE]
  WallQuantities | quantities | on 4 objects (4 IFCWALLSTANDARDCASE)
    GrossFootprintArea = 2. [SQUARE_METRE]
    GrossSideArea = 17.5 [SQUARE_METRE]
    GrossSideAreaLeft = 17.5 [SQUARE_METRE]
    GrossVolume = 7. [CUBIC_METRE]
    NetSideArea = 17.5 [SQUARE_METRE]
    NetSideAreaLeft = 17.5 [SQUARE_METRE]
    NetVolume = 7. [CUBIC_METRE]
    NominalHeight = 3.5 [METRE]
    NominalLength = 5. [METRE]
    NominalWidth = 0.4 [METRE]
  WallQuantities | quantities | on 4 objects (4 IFCWALLSTANDARDCASE)
    GrossFootprintArea = 3.84 [SQUARE_METRE]
    GrossSideArea = 33.6 [SQUARE_METRE]
    GrossSideAreaLeft = 33.6 [SQUARE_METRE]
    GrossVolume = 13.44 [CUBIC_METRE]
    NetSideArea = 30.926 [SQUARE_METRE]
    NetSideAreaLeft = 30.926 [SQUARE_METRE]
    NetVolume = 12.37 [CUBIC_METRE]
    NominalHeight = 3.5 [METRE]
    NominalLength = 9.6 [METRE]
    NominalWidth = 0.4 [METRE]
  WallQuantities | quantities | on 3 objects (3 IFCWALLSTANDARDCASE)
    GrossFootprintArea = 0.96 [SQUARE_METRE]
    GrossSideArea = 17.76 [SQUARE_METRE]
    GrossSideAreaLeft = 17.76 [SQUARE_METRE]
    GrossVolume = 3.552 [CUBIC_METRE]
    NetSideArea = 17.76 [SQUARE_METRE]
    NetSideAreaLeft = 17.76 [SQUARE_METRE]
    NetVolume = 3.552 [CUBIC_METRE]
    NominalHeight = 3.7 [METRE]
    NominalLength = 4.8 [METRE]
    NominalWidth = 0.2 [METRE]
  WallQuantities: 25 more contents on 33 objects not shown
  OpeningElementQuantities | quantities | on 24 objects (24 IFCOPENINGELEMENT)
    NominalArea = 2.674 [SQUARE_METRE]
    NominalVolume = 0.535 [CUBIC_METRE]
  OpeningElementQuantities | quantities | on 12 objects (12 IFCOPENINGELEMENT)
    NominalArea = 2.674 [SQUARE_METRE]
    NominalVolume = 1.07 [CUBIC_METRE]
  OpeningElementQuantities | quantities | on 10 objects (10 IFCOPENINGELEMENT)
    NominalArea = 3.604 [SQUARE_METRE]
    NominalVolume = 0.541 [CUBIC_METRE]
  OpeningElementQuantities | quantities | on 4 objects (4 IFCOPENINGELEMENT)
    NominalArea = 10.08 [SQUARE_METRE]
    NominalVolume = 2.016 [CUBIC_METRE]
  OpeningElementQuantities | quantities | on 4 objects (4 IFCOPENINGELEMENT)
    NominalArea = 2.384 [SQUARE_METRE]
    NominalVolume = 0.358 [CUBIC_METRE]
  OpeningElementQuantities | quantities | on 3 objects (3 IFCOPENINGELEMENT)
    NominalArea = 9. [SQUARE_METRE]
    NominalVolume = 1.8 [CUBIC_METRE]
  OpeningElementQuantities | quantities | on 3 objects (3 IFCOPENINGELEMENT)
    NominalArea = 8.97 [SQUARE_METRE]
    NominalVolume = 1.794 [CUBIC_METRE]
  OpeningElementQuantities | quantities | on 1 object (1 IFCOPENINGELEMENT)
    NominalArea = 10.08 [SQUARE_METRE]
    NominalVolume = 3.024 [CUBIC_METRE]
  OpeningElementQuantities: 5 more contents on 5 objects not shown
  Pset_ColumnCommon | properties | on 80 objects (80 IFCCOLUMN)
    FireRating = "F90" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "ST_OG_RECK" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 36 objects (36 IFCCOLUMN)
    FireRating = "F90" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "ST_OG_RECKL" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 20 objects (20 IFCCOLUMN)
    FireRating = "F90" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "ST_EG_RECK" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 9 objects (9 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "ST_KL_BET" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 9 objects (9 IFCCOLUMN)
    FireRating = "F90" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "ST_EG_RECKL" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  ColumnQuantities | quantities | on 80 objects (80 IFCCOLUMN)
    CrossSectionArea = 0.16 [SQUARE_METRE]
    GrossVolume = 0.496 [CUBIC_METRE]
    NetVolume = 0.496 [CUBIC_METRE]
    NominalHeight = 3.1 [METRE]
    OuterSurfaceArea = 5.28 [SQUARE_METRE]
  ColumnQuantities | quantities | on 36 objects (36 IFCCOLUMN)
    CrossSectionArea = 0.16 [SQUARE_METRE]
    GrossVolume = 0.56 [CUBIC_METRE]
    NetVolume = 0.56 [CUBIC_METRE]
    NominalHeight = 3.5 [METRE]
    OuterSurfaceArea = 5.92 [SQUARE_METRE]
  ColumnQuantities | quantities | on 20 objects (20 IFCCOLUMN)
    CrossSectionArea = 0.16 [SQUARE_METRE]
    GrossVolume = 0.72 [CUBIC_METRE]
    NetVolume = 0.72 [CUBIC_METRE]
    NominalHeight = 4.5 [METRE]
    OuterSurfaceArea = 7.52 [SQUARE_METRE]
  ColumnQuantities | quantities | on 9 objects (9 IFCCOLUMN)
    CrossSectionArea = 0.16 [SQUARE_METRE]
    GrossVolume = 0.416 [CUBIC_METRE]
    NetVolume = 0.416 [CUBIC_METRE]
    NominalHeight = 2.6 [METRE]
    OuterSurfaceArea = 4.48 [SQUARE_METRE]
  ColumnQuantities | quantities | on 9 objects (9 IFCCOLUMN)
    CrossSectionArea = 0.16 [SQUARE_METRE]
    GrossVolume = 0.784 [CUBIC_METRE]
    NetVolume = 0.784 [CUBIC_METRE]
    NominalHeight = 4.9 [METRE]
    OuterSurfaceArea = 8.16 [SQUARE_METRE]
  Pset_StairCommon | properties | on 2 objects (2 IFCSTAIR)
    FireExit = TRUE (IFCBOOLEAN)
    FireRating = "F90" (IFCLABEL)
    HandicapAccessible = FALSE (IFCBOOLEAN)
    HasNonSkidSurface = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 20. (IFCCOUNTMEASURE)
    RequiredHeadroom = 2.5 (IFCPOSITIVELENGTHMEASURE) [METRE]
    RiserHeight = 180. (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 239.99 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    FireExit = TRUE (IFCBOOLEAN)
    FireRating = "F90" (IFCLABEL)
    HandicapAccessible = FALSE (IFCBOOLEAN)
    HasNonSkidSurface = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 18. (IFCCOUNTMEASURE)
    Reference = "TR_FT_KL" (IFCIDENTIFIER)
    RequiredHeadroom = 0. (IFCPOSITIVELENGTHMEASURE) [METRE]
    RiserHeight = 172.222222222222 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 260. (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    FireExit = TRUE (IFCBOOLEAN)
    FireRating = "F90" (IFCLABEL)
    HandicapAccessible = FALSE (IFCBOOLEAN)
    HasNonSkidSurface = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 14. (IFCCOUNTMEASURE)
    Reference = "FT_TREPP_EG" (IFCIDENTIFIER)
    RequiredHeadroom = 0. (IFCPOSITIVELENGTHMEASURE) [METRE]
    RiserHeight = 180. (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 242.842857142857 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 14. (IFCCOUNTMEASURE)
    RiserHeight = 180. (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 242.842857142857 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    FireExit = TRUE (IFCBOOLEAN)
    FireRating = "F90" (IFCLABEL)
    HandicapAccessible = FALSE (IFCBOOLEAN)
    HasNonSkidSurface = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 20. (IFCCOUNTMEASURE)
    Reference = "FT_TR" (IFCIDENTIFIER)
    RequiredHeadroom = 2.5 (IFCPOSITIVELENGTHMEASURE) [METRE]
    RiserHeight = 180. (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 239.99 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_ManufacturerTypeInformation | properties | on 200 objects (200 IFCCURTAINWALL)
    Manufacturer = "GARFAG" (IFCLABEL)
    ModelLabel = "GLT_FAS" (IFCLABEL)
    ModelReference = "0.000000" (IFCLABEL)
    ProductionYear = "2019" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 18 objects (18 IFCCURTAINWALL)
    Manufacturer = "GARFAG" (IFCLABEL)
    ModelLabel = "ALTA" (IFCLABEL)
    ModelReference = "0.000000" (IFCLABEL)
    ProductionYear = "2019" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 14 objects (14 IFCDOOR)
    ArticleNumber = "TGT_OLH" (IFCIDENTIFIER)
    Manufacturer = "DOMAG" (IFCLABEL)
    ModelLabel = "DO_BLANK" (IFCLABEL)
    ModelReference = "1101.000000" (IFCLABEL)
    ProductionYear = "2019" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 6 objects (6 IFCSLAB)
    ProductionYear = "2020" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCELEMENTASSEMBLY)
    ArticleNumber = "1001" (IFCIDENTIFIER)
    Manufacturer = "DEGRA" (IFCLABEL)
    ModelLabel = "ET_FASS" (IFCLABEL)
    ModelReference = "1001.000000" (IFCLABEL)
    ProductionYear = "2010" (IFCLABEL)
  Pset_OpeningElementCommon | properties | on 11 objects (11 IFCOPENINGELEMENT)
    ProtectedOpening = FALSE (IFCBOOLEAN)
    Purpose = "TR" (IFCLABEL)
    Reference = "DD" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 5 objects (5 IFCOPENINGELEMENT)
    ProtectedOpening = FALSE (IFCBOOLEAN)
    Purpose = "AUFZ" (IFCLABEL)
  Pset_BeamCommon | properties | on 10 objects (10 IFCBEAM)
    FireRating = "F90" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "UZ_LANG" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 30. (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon | properties | on 10 objects (10 IFCBEAM)
    FireRating = "F90" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "UZ_KURZ" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 15. (IFCPOSITIVELENGTHMEASURE) [METRE]
  BeamQuantities | quantities | on 10 objects (10 IFCBEAM)
    CrossSectionArea = 0.16 [SQUARE_METRE]
    GrossVolume = 4.864 [CUBIC_METRE]
    NetVolume = 4.864 [CUBIC_METRE]
    NominalLength = 30.4 [METRE]
    OuterSurfaceArea = 48.96 [SQUARE_METRE]
  BeamQuantities | quantities | on 10 objects (10 IFCBEAM)
    CrossSectionArea = 0.16 [SQUARE_METRE]
    GrossVolume = 3.136 [CUBIC_METRE]
    NetVolume = 3.136 [CUBIC_METRE]
    NominalLength = 19.6 [METRE]
    OuterSurfaceArea = 31.68 [SQUARE_METRE]
  Pset_CurtainWallCommon | properties | on 200 objects (200 IFCCURTAINWALL)
    AcousticRating = "5" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    FireRating = "F90" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "GLATA_001" (IFCIDENTIFIER)
    SurfaceSpreadOfFlame = "A" (IFCLABEL)
    ThermalTransmittance = 0.25 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_CurtainWallCommon | properties | on 6 objects (6 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_CurtainWallCommon | properties | on 3 objects (3 IFCCURTAINWALL)
    AcousticRating = "5" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    FireRating = "F90" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "FASS_TAFEL_LANG_SU" (IFCIDENTIFIER)
    SurfaceSpreadOfFlame = "A" (IFCLABEL)
    ThermalTransmittance = 0.45 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_CurtainWallCommon | properties | on 3 objects (3 IFCCURTAINWALL)
    AcousticRating = "5" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    FireRating = "F90" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "FASS_TAFEL_KUR_WE" (IFCIDENTIFIER)
    SurfaceSpreadOfFlame = "A" (IFCLABEL)
    ThermalTransmittance = 0.45 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_CurtainWallCommon | properties | on 3 objects (3 IFCCURTAINWALL)
    AcousticRating = "5" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    FireRating = "F90" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "FASS_TAFKL_LANG_SU" (IFCIDENTIFIER)
    SurfaceSpreadOfFlame = "A" (IFCLABEL)
    ThermalTransmittance = 0.45 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_CurtainWallCommon | properties | on 3 objects (3 IFCCURTAINWALL)
    AcousticRating = "5" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    FireRating = "F90" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "FASS_TAFKL_KUR_WE" (IFCIDENTIFIER)
    SurfaceSpreadOfFlame = "A" (IFCLABEL)
    ThermalTransmittance = 0.45 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_CurtainWallCommon | properties | on 2 objects (2 IFCCURTAINWALL)
    AcousticRating = "5" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    FireRating = "F90" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "FASS_PAN_KUR_DA" (IFCIDENTIFIER)
    SurfaceSpreadOfFlame = "A" (IFCLABEL)
    ThermalTransmittance = 0.45 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_CurtainWallCommon | properties | on 2 objects (2 IFCCURTAINWALL)
    AcousticRating = "5" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    FireRating = "F90" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "FASS_PAN_LANG_DA" (IFCIDENTIFIER)
    SurfaceSpreadOfFlame = "A" (IFCLABEL)
    ThermalTransmittance = 0.45 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_CurtainWallCommon: 2 more contents on 2 objects not shown
  AllplanAttributes (1flg Weiß Oberlicht) | properties | on 1 object (1 IFCDOOR)
    Allright_Bauteil_ID = "2405Mak0000004509" (IFCTEXT)
    Antrieb = FALSE (IFCBOOLEAN)
    Beanspruchungsgruppe = "M" (IFCTEXT)
    Bezeichnung = "1flg Weiß Oberlicht" (IFCTEXT)
    Einheit = "m³" (IFCTEXT)
    Erdreich = "no" (IFCTEXT)
    Gewerk = "" (IFCTEXT)
    Glasanteil_berücksichtigen = 0 (IFCINTEGER)
    Glasart = "normal" (IFCTEXT)
    Klimaklasse = "I" (IFCTEXT)
    Material = "Innentür" (IFCTEXT)
    MechanicalLoadRating = "4" (IFCTEXT)
    Objektname = "Türmakro, -SmartPart" (IFCTEXT)
    Plugin_Bezeichnung = "MainObject" (IFCTEXT)
    Plugin_Objektname = "SmartPartCompressed" (IFCTEXT)
    Programmversion = "3.0" (IFCTEXT)
    Typ = "Innentür" (IFCTEXT)
    Umbaukategorie = "Neubau" (IFCTEXT)
    V6 = 0. (IFCREAL)
    V7 = 0. (IFCREAL)
    V8 = 0. (IFCREAL)
    V9 = 0. (IFCREAL)
    Verschattung = 0 (IFCINTEGER)
    Version = "6.0" (IFCTEXT)
    WaterTightnessRating = "0" (IFCTEXT)
    WindLoadRating = "5" (IFCTEXT)
  AllplanAttributes (1flg Weiß Oberlicht) | properties | on 1 object (1 IFCDOOR)
    Allright_Bauteil_ID = "2405Mak0000004511" (IFCTEXT)
    Antrieb = FALSE (IFCBOOLEAN)
    Beanspruchungsgruppe = "M" (IFCTEXT)
    Bezeichnung = "1flg Weiß Oberlicht" (IFCTEXT)
    Einheit = "m³" (IFCTEXT)
    Erdreich = "no" (IFCTEXT)
    Gewerk = "" (IFCTEXT)
    Glasanteil_berücksichtigen = 0 (IFCINTEGER)
    Glasart = "normal" (IFCTEXT)
    Klimaklasse = "I" (IFCTEXT)
    Material = "Innentür" (IFCTEXT)
    MechanicalLoadRating = "4" (IFCTEXT)
    Objektname = "Türmakro, -SmartPart" (IFCTEXT)
    Plugin_Bezeichnung = "MainObject" (IFCTEXT)
    Plugin_Objektname = "SmartPartCompressed" (IFCTEXT)
    Programmversion = "3.0" (IFCTEXT)
    Typ = "Innentür" (IFCTEXT)
    Umbaukategorie = "Neubau" (IFCTEXT)
    V6 = 0. (IFCREAL)
    V7 = 0. (IFCREAL)
    V8 = 0. (IFCREAL)
    V9 = 0. (IFCREAL)
    Verschattung = 0 (IFCINTEGER)
    Version = "6.0" (IFCTEXT)
    WaterTightnessRating = "0" (IFCTEXT)
    WindLoadRating = "5" (IFCTEXT)
  AllplanAttributes (1flg Weiß Oberlicht) | properties | on 1 object (1 IFCDOOR)
    Allright_Bauteil_ID = "2405Mak0000004513" (IFCTEXT)
    Antrieb = FALSE (IFCBOOLEAN)
    Beanspruchungsgruppe = "M" (IFCTEXT)
    Bezeichnung = "1flg Weiß Oberlicht" (IFCTEXT)
    Einheit = "m³" (IFCTEXT)
    Erdreich = "no" (IFCTEXT)
    Gewerk = "" (IFCTEXT)
    Glasanteil_berücksichtigen = 0 (IFCINTEGER)
    Glasart = "normal" (IFCTEXT)
    Klimaklasse = "I" (IFCTEXT)
    Material = "Innentür" (IFCTEXT)
    MechanicalLoadRating = "4" (IFCTEXT)
    Objektname = "Türmakro, -SmartPart" (IFCTEXT)
    Plugin_Bezeichnung = "MainObject" (IFCTEXT)
    Plugin_Objektname = "SmartPartCompressed" (IFCTEXT)
    Programmversion = "3.0" (IFCTEXT)
    Typ = "Innentür" (IFCTEXT)
    Umbaukategorie = "Neubau" (IFCTEXT)
    V6 = 0. (IFCREAL)
    V7 = 0. (IFCREAL)
    V8 = 0. (IFCREAL)
    V9 = 0. (IFCREAL)
    Verschattung = 0 (IFCINTEGER)
    Version = "6.0" (IFCTEXT)
    WaterTightnessRating = "0" (IFCTEXT)
    WindLoadRating = "5" (IFCTEXT)
  AllplanAttributes (1flg Weiß Oberlicht) | properties | on 1 object (1 IFCDOOR)
    Allright_Bauteil_ID = "2405Mak0000004515" (IFCTEXT)
    Antrieb = FALSE (IFCBOOLEAN)
    Beanspruchungsgruppe = "M" (IFCTEXT)
    Bezeichnung = "1flg Weiß Oberlicht" (IFCTEXT)
    Einheit = "m³" (IFCTEXT)
    Erdreich = "no" (IFCTEXT)
    Glasanteil_berücksichtigen = 0 (IFCINTEGER)
    Glasart = "normal" (IFCTEXT)
    Klimaklasse = "I" (IFCTEXT)
    Material = "Innentür" (IFCTEXT)
    MechanicalLoadRating = "4" (IFCTEXT)
    Objektname = "Türmakro, -SmartPart" (IFCTEXT)
    Plugin_Bezeichnung = "MainObject" (IFCTEXT)
    Plugin_Objektname = "SmartPartCompressed" (IFCTEXT)
    Programmversion = "3.0" (IFCTEXT)
    Typ = "Innentür" (IFCTEXT)
    Umbaukategorie = "Neubau" (IFCTEXT)
    V6 = 0. (IFCREAL)
    V7 = 0. (IFCREAL)
    V8 = 0. (IFCREAL)
    V9 = 0. (IFCREAL)
    Verschattung = 0 (IFCINTEGER)
    Version = "6.0" (IFCTEXT)
    WaterTightnessRating = "0" (IFCTEXT)
    WindLoadRating = "5" (IFCTEXT)
  AllplanAttributes (1flg Weiß Oberlicht) | properties | on 1 object (1 IFCDOOR)
    Allright_Bauteil_ID = "2405Mak0000004521" (IFCTEXT)
    Antrieb = FALSE (IFCBOOLEAN)
    Beanspruchungsgruppe = "M" (IFCTEXT)
    Bezeichnung = "1flg Weiß Oberlicht" (IFCTEXT)
    Einheit = "m³" (IFCTEXT)
    Erdreich = "no" (IFCTEXT)
    Glasanteil_berücksichtigen = 0 (IFCINTEGER)
    Glasart = "normal" (IFCTEXT)
    Klimaklasse = "I" (IFCTEXT)
    Material = "Innentür" (IFCTEXT)
    MechanicalLoadRating = "4" (IFCTEXT)
    Objektname = "Türmakro, -SmartPart" (IFCTEXT)
    Plugin_Bezeichnung = "MainObject" (IFCTEXT)
    Plugin_Objektname = "SmartPartCompressed" (IFCTEXT)
    Programmversion = "3.0" (IFCTEXT)
    Typ = "Innentür" (IFCTEXT)
    Umbaukategorie = "Neubau" (IFCTEXT)
    V6 = 0. (IFCREAL)
    V7 = 0. (IFCREAL)
    V8 = 0. (IFCREAL)
    V9 = 0. (IFCREAL)
    Verschattung = 0 (IFCINTEGER)
    Version = "6.0" (IFCTEXT)
    WaterTightnessRating = "0" (IFCTEXT)
    WindLoadRating = "5" (IFCTEXT)
  AllplanAttributes (1flg Weiß Oberlicht) | properties | on 1 object (1 IFCDOOR)
    Allright_Bauteil_ID = "2505Mak0000000073" (IFCTEXT)
    Antrieb = FALSE (IFCBOOLEAN)
    Beanspruchungsgruppe = "M" (IFCTEXT)
    Bezeichnung = "1flg Weiß Oberlicht" (IFCTEXT)
    Einheit = "m³" (IFCTEXT)
    Erdreich = "no" (IFCTEXT)
    Gewerk = "" (IFCTEXT)
    Glasanteil_berücksichtigen = 0 (IFCINTEGER)
    Glasart = "normal" (IFCTEXT)
    Klimaklasse = "I" (IFCTEXT)
    Material = "Innentür" (IFCTEXT)
    MechanicalLoadRating = "4" (IFCTEXT)
    Objektname = "Türmakro, -SmartPart" (IFCTEXT)
    Plugin_Bezeichnung = "MainObject" (IFCTEXT)
    Plugin_Objektname = "SmartPartCompressed" (IFCTEXT)
    Programmversion = "3.0" (IFCTEXT)
    Typ = "Innentür" (IFCTEXT)
    Umbaukategorie = "Neubau" (IFCTEXT)
    V6 = 0. (IFCREAL)
    V7 = 0. (IFCREAL)
    V8 = 0. (IFCREAL)
    V9 = 0. (IFCREAL)
    Verschattung = 0 (IFCINTEGER)
    Version = "6.0" (IFCTEXT)
    WaterTightnessRating = "0" (IFCTEXT)
    WindLoadRating = "5" (IFCTEXT)
  AllplanAttributes (1flg Weiß Oberlicht) | properties | on 1 object (1 IFCDOOR)
    Allright_Bauteil_ID = "2505Mak0000000071" (IFCTEXT)
    Antrieb = FALSE (IFCBOOLEAN)
    Beanspruchungsgruppe = "M" (IFCTEXT)
    Bezeichnung = "1flg Weiß Oberlicht" (IFCTEXT)
    Einheit = "m³" (IFCTEXT)
    Erdreich = "no" (IFCTEXT)
    Glasanteil_berücksichtigen = 0 (IFCINTEGER)
    Glasart = "normal" (IFCTEXT)
    Klimaklasse = "I" (IFCTEXT)
    Material = "Innentür" (IFCTEXT)
    MechanicalLoadRating = "4" (IFCTEXT)
    Objektname = "Türmakro, -SmartPart" (IFCTEXT)
    Plugin_Bezeichnung = "MainObject" (IFCTEXT)
    Plugin_Objektname = "SmartPartCompressed" (IFCTEXT)
    Programmversion = "3.0" (IFCTEXT)
    Typ = "Innentür" (IFCTEXT)
    Umbaukategorie = "Neubau" (IFCTEXT)
    V6 = 0. (IFCREAL)
    V7 = 0. (IFCREAL)
    V8 = 0. (IFCREAL)
    V9 = 0. (IFCREAL)
    Verschattung = 0 (IFCINTEGER)
    Version = "6.0" (IFCTEXT)
    WaterTightnessRating = "0" (IFCTEXT)
    WindLoadRating = "5" (IFCTEXT)
  AllplanAttributes (1flg Weiß Oberlicht) | properties | on 1 object (1 IFCDOOR)
    Allright_Bauteil_ID = "2505Mak0000000065" (IFCTEXT)
    Antrieb = FALSE (IFCBOOLEAN)
    Beanspruchungsgruppe = "M" (IFCTEXT)
    Bezeichnung = "1flg Weiß Oberlicht" (IFCTEXT)
    Einheit = "m³" (IFCTEXT)
    Erdreich = "no" (IFCTEXT)
    Glasanteil_berücksichtigen = 0 (IFCINTEGER)
    Glasart = "normal" (IFCTEXT)
    Klimaklasse = "I" (IFCTEXT)
    Material = "Innentür" (IFCTEXT)
    MechanicalLoadRating = "4" (IFCTEXT)
    Objektname = "Türmakro, -SmartPart" (IFCTEXT)
    Plugin_Bezeichnung = "MainObject" (IFCTEXT)
    Plugin_Objektname = "SmartPartCompressed" (IFCTEXT)
    Programmversion = "3.0" (IFCTEXT)
    Typ = "Innentür" (IFCTEXT)
    Umbaukategorie = "Neubau" (IFCTEXT)
    V6 = 0. (IFCREAL)
    V7 = 0. (IFCREAL)
    V8 = 0. (IFCREAL)
    V9 = 0. (IFCREAL)
    Verschattung = 0 (IFCINTEGER)
    Version = "6.0" (IFCTEXT)
    WaterTightnessRating = "0" (IFCTEXT)
    WindLoadRating = "5" (IFCTEXT)
  AllplanAttributes (1flg Weiß Oberlicht): 2 more contents on 2 objects not shown
  Pset_DoorCommon | properties | on 14 objects (14 IFCDOOR)
    AcousticRating = "5" (IFCLABEL)
    FireExit = TRUE (IFCBOOLEAN)
    FireRating = "F90" (IFCLABEL)
    HandicapAccessible = FALSE (IFCBOOLEAN)
    Infiltration = 35. (IFCVOLUMETRICFLOWRATEMEASURE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "TR_TUER_GK" (IFCIDENTIFIER)
    SecurityRating = "SA" (IFCLABEL)
    SelfClosing = TRUE (IFCBOOLEAN)
    SmokeStop = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0.66 (IFCTHERMALTRANSMITTANCEMEASURE)
  AllplanAttributes (Türöffnung) | properties | on 1 object (1 IFCDOOR)
    Allright_Bauteil_ID = "2405Mak0000004517" (IFCTEXT)
    Antrieb = FALSE (IFCBOOLEAN)
    Beanspruchungsgruppe = "M" (IFCTEXT)
    Bezeichnung = "Türöffnung" (IFCTEXT)
    Einheit = "m²" (IFCTEXT)
    Erdreich = "no" (IFCTEXT)
    Gewerk = "" (IFCTEXT)
    Glasanteil_berücksichtigen = 0 (IFCINTEGER)
    Glasart = "normal" (IFCTEXT)
    Klimaklasse = "I" (IFCTEXT)
    Material = "Innentür" (IFCTEXT)
    MechanicalLoadRating = "4" (IFCTEXT)
    Objektname = "Türöffnung" (IFCTEXT)
    Plugin_Bezeichnung = "MainObject" (IFCTEXT)
    Plugin_Objektname = "SmartPartCompressed" (IFCTEXT)
    Programmversion = "3.0" (IFCTEXT)
    Typ = "Innentür" (IFCTEXT)
    Umbaukategorie = "Neubau" (IFCTEXT)
    V6 = 0. (IFCREAL)
    V7 = 0. (IFCREAL)
    V8 = 0. (IFCREAL)
    V9 = 0. (IFCREAL)
    Verschattung = 0 (IFCINTEGER)
    Version = "6.0" (IFCTEXT)
    WaterTightnessRating = "0" (IFCTEXT)
    WindLoadRating = "5" (IFCTEXT)
  AllplanAttributes (Türöffnung) | properties | on 1 object (1 IFCDOOR)
    Allright_Bauteil_ID = "2405Mak0000004519" (IFCTEXT)
    Antrieb = FALSE (IFCBOOLEAN)
    Beanspruchungsgruppe = "M" (IFCTEXT)
    Bezeichnung = "Türöffnung" (IFCTEXT)
    Einheit = "m²" (IFCTEXT)
    Erdreich = "no" (IFCTEXT)
    Gewerk = "" (IFCTEXT)
    Glasanteil_berücksichtigen = 0 (IFCINTEGER)
    Glasart = "normal" (IFCTEXT)
    Klimaklasse = "I" (IFCTEXT)
    Material = "Innentür" (IFCTEXT)
    MechanicalLoadRating = "4" (IFCTEXT)
    Objektname = "Türöffnung" (IFCTEXT)
    Plugin_Bezeichnung = "MainObject" (IFCTEXT)
    Plugin_Objektname = "SmartPartCompressed" (IFCTEXT)
    Programmversion = "3.0" (IFCTEXT)
    Typ = "Innentür" (IFCTEXT)
    Umbaukategorie = "Neubau" (IFCTEXT)
    V6 = 0. (IFCREAL)
    V7 = 0. (IFCREAL)
    V8 = 0. (IFCREAL)
    V9 = 0. (IFCREAL)
    Verschattung = 0 (IFCINTEGER)
    Version = "6.0" (IFCTEXT)
    WaterTightnessRating = "0" (IFCTEXT)
    WindLoadRating = "5" (IFCTEXT)
  AllplanAttributes (Türöffnung) | properties | on 1 object (1 IFCDOOR)
    Allright_Bauteil_ID = "2505Mak0000000067" (IFCTEXT)
    Antrieb = FALSE (IFCBOOLEAN)
    Beanspruchungsgruppe = "M" (IFCTEXT)
    Bezeichnung = "Türöffnung" (IFCTEXT)
    Einheit = "m²" (IFCTEXT)
    Erdreich = "no" (IFCTEXT)
    Gewerk = "" (IFCTEXT)
    Glasanteil_berücksichtigen = 0 (IFCINTEGER)
    Glasart = "normal" (IFCTEXT)
    Klimaklasse = "I" (IFCTEXT)
    Material = "Innentür" (IFCTEXT)
    MechanicalLoadRating = "4" (IFCTEXT)
    Objektname = "Türöffnung" (IFCTEXT)
    Plugin_Bezeichnung = "MainObject" (IFCTEXT)
    Plugin_Objektname = "SmartPartCompressed" (IFCTEXT)
    Programmversion = "3.0" (IFCTEXT)
    Typ = "Innentür" (IFCTEXT)
    Umbaukategorie = "Neubau" (IFCTEXT)
    V6 = 0. (IFCREAL)
    V7 = 0. (IFCREAL)
    V8 = 0. (IFCREAL)
    V9 = 0. (IFCREAL)
    Verschattung = 0 (IFCINTEGER)
    Version = "6.0" (IFCTEXT)
    WaterTightnessRating = "0" (IFCTEXT)
    WindLoadRating = "5" (IFCTEXT)
  AllplanAttributes (Türöffnung) | properties | on 1 object (1 IFCDOOR)
    Allright_Bauteil_ID = "2505Mak0000000069" (IFCTEXT)
    Antrieb = FALSE (IFCBOOLEAN)
    Beanspruchungsgruppe = "M" (IFCTEXT)
    Bezeichnung = "Türöffnung" (IFCTEXT)
    Einheit = "m²" (IFCTEXT)
    Erdreich = "no" (IFCTEXT)
    Gewerk = "" (IFCTEXT)
    Glasanteil_berücksichtigen = 0 (IFCINTEGER)
    Glasart = "normal" (IFCTEXT)
    Klimaklasse = "I" (IFCTEXT)
    Material = "Innentür" (IFCTEXT)
    MechanicalLoadRating = "4" (IFCTEXT)
    Objektname = "Türöffnung" (IFCTEXT)
    Plugin_Bezeichnung = "MainObject" (IFCTEXT)
    Plugin_Objektname = "SmartPartCompressed" (IFCTEXT)
    Programmversion = "3.0" (IFCTEXT)
    Typ = "Innentür" (IFCTEXT)
    Umbaukategorie = "Neubau" (IFCTEXT)
    V6 = 0. (IFCREAL)
    V7 = 0. (IFCREAL)
    V8 = 0. (IFCREAL)
    V9 = 0. (IFCREAL)
    Verschattung = 0 (IFCINTEGER)
    Version = "6.0" (IFCTEXT)
    WaterTightnessRating = "0" (IFCTEXT)
    WindLoadRating = "5" (IFCTEXT)
  SpaceQuantities | quantities | on 4 objects (4 IFCSPACE)
    ClearHeight = 3.25 [METRE]
    GrossFloorArea = 11.347 [SQUARE_METRE]
    GrossVolume = 39.716 [CUBIC_METRE]
    GrossWallArea = 51.275 [SQUARE_METRE]
    NetFloorArea = 11.348 [SQUARE_METRE]
    NetPerimeter = 14.65 [METRE]
    NetVolume = 36.879 [CUBIC_METRE]
    NetWallArea = 48.892 [SQUARE_METRE]
    NominalHeight = 3.5 [METRE]
  SpaceQuantities | quantities | on 2 objects (2 IFCSPACE)
    ClearHeight = 3.5 [METRE]
    GrossFloorArea = 97.023 [SQUARE_METRE]
    GrossVolume = 339.579 [CUBIC_METRE]
    GrossWallArea = 137.9 [SQUARE_METRE]
    NetFloorArea = 97.023 [SQUARE_METRE]
    NetPerimeter = 39.4 [METRE]
    NetVolume = 339.579 [CUBIC_METRE]
    NetWallArea = 134.296 [SQUARE_METRE]
    NominalHeight = 3.5 [METRE]
  SpaceQuantities | quantities | on 2 objects (2 IFCSPACE)
    ClearHeight = 3.5 [METRE]
    GrossFloorArea = 92.16 [SQUARE_METRE]
    GrossVolume = 322.56 [CUBIC_METRE]
    GrossWallArea = 134.4 [SQUARE_METRE]
    NetFloorArea = 92.16 [SQUARE_METRE]
    NetPerimeter = 38.4 [METRE]
    NetVolume = 322.56 [CUBIC_METRE]
    NetWallArea = 100.281 [SQUARE_METRE]
    NominalHeight = 3.5 [METRE]
  SpaceQuantities | quantities | on 2 objects (2 IFCSPACE)
    ClearHeight = 3.5 [METRE]
    GrossFloorArea = 69. [SQUARE_METRE]
    GrossVolume = 241.5 [CUBIC_METRE]
    GrossWallArea = 137.2 [SQUARE_METRE]
    NetFloorArea = 69. [SQUARE_METRE]
    NetPerimeter = 39.2 [METRE]
    NetVolume = 241.5 [CUBIC_METRE]
    NetWallArea = 105. [SQUARE_METRE]
    NominalHeight = 3.5 [METRE]
  SpaceQuantities | quantities | on 2 objects (2 IFCSPACE)
    ClearHeight = 3.5 [METRE]
    GrossFloorArea = 69. [SQUARE_METRE]
    GrossVolume = 241.5 [CUBIC_METRE]
    GrossWallArea = 137.2 [SQUARE_METRE]
    NetFloorArea = 69. [SQUARE_METRE]
    NetPerimeter = 39.2 [METRE]
    NetVolume = 241.5 [CUBIC_METRE]
    NetWallArea = 116.333 [SQUARE_METRE]
    NominalHeight = 3.5 [METRE]
  SpaceQuantities | quantities | on 2 objects (2 IFCSPACE)
    ClearHeight = 3.5 [METRE]
    GrossFloorArea = 22.31 [SQUARE_METRE]
    GrossVolume = 78.085 [CUBIC_METRE]
    GrossWallArea = 66.15 [SQUARE_METRE]
    NetFloorArea = 22.31 [SQUARE_METRE]
    NetPerimeter = 18.9 [METRE]
    NetVolume = 78.085 [CUBIC_METRE]
    NetWallArea = 62.546 [SQUARE_METRE]
    NominalHeight = 3.5 [METRE]
  SpaceQuantities | quantities | on 2 objects (2 IFCSPACE)
    ClearHeight = 3.5 [METRE]
    GrossFloorArea = 23.523 [SQUARE_METRE]
    GrossVolume = 82.329 [CUBIC_METRE]
    GrossWallArea = 67.9 [SQUARE_METRE]
    NetFloorArea = 23.523 [SQUARE_METRE]
    NetPerimeter = 19.4 [METRE]
    NetVolume = 82.329 [CUBIC_METRE]
    NetWallArea = 64.296 [SQUARE_METRE]
    NominalHeight = 3.5 [METRE]
  SpaceQuantities | quantities | on 2 objects (2 IFCSPACE)
    ClearHeight = 3.5 [METRE]
    GrossFloorArea = 23.522 [SQUARE_METRE]
    GrossVolume = 82.329 [CUBIC_METRE]
    GrossWallArea = 67.9 [SQUARE_METRE]
    NetFloorArea = 23.523 [SQUARE_METRE]
    NetPerimeter = 19.4 [METRE]
    NetVolume = 82.329 [CUBIC_METRE]
    NetWallArea = 64.296 [SQUARE_METRE]
    NominalHeight = 3.5 [METRE]
  SpaceQuantities: 11 more contents on 14 objects not shown
  CoveringQuantities | quantities | on 4 objects (4 IFCCOVERING)
    NetArea = 11.399 [SQUARE_METRE]
  CoveringQuantities | quantities | on 1 object (1 IFCCOVERING)
    NetArea = 1210. [SQUARE_METRE]
  PsetCoveringCommon | properties | on 1 object (1 IFCCOVERING)
    Flammability = "A" (IFCLABEL)