Kernel driver max6650
=====================

Supported chips:
  * Maxim 6650 / 6651
    Prefix: 'max6650'
    Addresses scanned: I2C 0x1b, 0x1f, 0x48, 0x4b
    Datasheet: http://pdfserv.maxim-ic.com/en/ds/MAX6650-MAX6651.pdf

Authors:
    Hans J. Koch <hjk@hansjkoch.de>
    John Morris <john.morris@spirentcom.com>
    Claus Gindhart <claus.gindhart@kontron.com>

Description
-----------

This driver implements support for the Maxim 6650/6651

The 2 devices are very similar, but the Maxim 6550 has a reduced feature
set, e.g. only one fan-input, instead of 4 for the 6651.

The driver is not able to distinguish between the 2 devices.

The driver provides the following sensor accesses in sysfs:

fan1_input	ro	fan tachometer speed in RPM
fan2_input	ro	"
fan3_input	ro	"
fan4_input	ro	"
fan1_target	rw	desired fan speed in RPM (closed loop mode only)
pwm1_enable	rw	regulator mode, 0=full on, 1=open loop, 2=closed loop
pwm1		rw	relative speed (0-255), 255=max. speed.
			Used in open loop mode only.
fan1_div	rw	sets the speed range the inputs can handle. Legal
			values are 1, 2, 4, and 8. Use lower values for
			faster fans.

Module parameters
-----------------

If your board has a BIOS that initializes the MAX6650/6651 correctly, you can
simply load your module without parameters. It won't touch the configuration
registers then. If your board BIOS doesn't initialize the chip, or you want
different settings, you can set the following parameters:

voltage_12V: 5=5V fan, 12=12V fan, 0=don't change
prescaler: Possible values are 1,2,4,8,16, or 0 for don't change
clock: The clock frequency in Hz of the chip the driver should assume [254000]

Please have a look at the MAX6650/6651 data sheet and make sure that you fully
understand the meaning of these parameters before you attempt to change them.

