Talk-A-Phone Co.
Model ETP-SMH Hooded Surface Mount Accessory
Architectural & Engineering Specification rev. 7/20/09

1	General Description

1.1	The unit shall be a highly vandal-resistant stainless steel emergency phone Hooded Surface Mount Accessory, model ETP-SMH, no substitutions, suitable for mounting on an outdoor wall or poll.  The Surface Mount shall house an ADA-compliant, line-powered communication device manufactured by Talk-A-Phone Co.  Externally-powered devices are not acceptable.

2	Construction

2.1	The unit shall be constructed of stainless steel and weigh approximately 7 lbs.

2.2	The unit shall measure 10.50" W x 12.75" H x 6.5" D (Top) x 5.0" D (Bottom).

2.3	The unit shall be painted in Safety Yellow with "EMERGENCY" emblazoned on both sides in reflective black vinyl letters.  Custom wording and colors shall be available.

2.4	The unit shall be designed such that any 400-Series flush mounting Emergency Phone shall recess mount into Hooded Surface Mount Accessory.

2.5	The unit shall have 7/8" conduit entry holes on back and bottom (or optionally on top)

3	Electrical

3.1	The communication device shall require no external power.  It shall be powered by the phone line, PBX extension, or a wireless communication interface.

4	Mounting

4.1	The Hooded Surface Mount shall have four 0.34" holes on the back wall for surface mounting on a wall or strapping to a poll.

4.2	Poll Mounting Kit, model ETP-PMKT, shall be available for strapping to a poll.

5	Options

5.1	Communications

5.1.1	Surface Mount shall accept any 400-Series flush mounting emergency phone.

5.1.2	Communication device shall accept fiber optic line instead of standard copper wire.  400-Series flush mounting emergency phone and fiber interface shall be required.

5.1.3	Cellular Interface shall be available when phone line is not available.
 
5.1.3.1	Transmission shall be tri mode 800MHz TDMA/1900 MHz PCS/800 MHz AMPS, model ETP-CI.

5.1.3.2	Transmission shall be 1900Mhz GSM, model ETP-CI/GSM.

5.1.4	Radio Frequency Interface, model ETP-WTR/1, shall be available when phone lines are not available.  Radio Frequency Interface functions as part of a complete proprietary radio frequency system.

6	Compliance

6.1	CSA Certified to UL Standard 60950

7	Warranty

7.1	Equipment shall be warrantied against any defects in material and workmanship, under normal use, for a period of one year from date of installation. In the event system is found by manufacturer to be defective within the warranty period, manufacturer shall repair and/or replace any defective parts, provided the equipment is returned to manufacturer.

8	Manufacturer

8.1	The Manufacturer shall be Talk-A-Phone Co. (773) 539-1100, 7530 N. Natchez Ave, Niles, Illinois 60714-3804, www.talkaphone.com.  THERE ARE NO EQUIVALENTS.